diff --git a/ixgbe/ixgbe_main.c b/ixgbe/ixgbe_main.c
index 30f9ccf..60c0252 100644
--- a/ixgbe/ixgbe_main.c
+++ b/ixgbe/ixgbe_main.c
@@ -221,6 +221,22 @@ static const struct ixgbe_reg_info ixgbe_reg_info_tbl[] = {
 	{}
 };
 
+#if defined(CONFIG_NETMAP) || defined(CONFIG_NETMAP_MODULE)
+/*
+ * The #ifdef DEV_NETMAP / #endif blocks in this file are meant to
+ * be a reference on how to implement netmap support in a driver.
+ * Additional comments are in ixgbe_netmap_linux.h .
+ *
+ * The code is originally developed on FreeBSD and in the interest
+ * of maintainability we try to limit differences between the two systems.
+ *
+ * <ixgbe_netmap_linux.h> contains functions for netmap support
+ * that extend the standard driver.
+ * It also defines DEV_NETMAP so further conditional sections use
+ * that instead of CONFIG_NETMAP
+ */
+#include <ixgbe_netmap_linux.h>
+#endif
 
 /*
  * ixgbe_regdump - register printout routine
@@ -826,6 +842,16 @@ static bool ixgbe_clean_tx_irq(struct ixgbe_q_vector *q_vector,
 	unsigned int total_bytes = 0, total_packets = 0;
 	u16 i, eop, count = 0;
 
+#ifdef DEV_NETMAP
+	/*
+	 * In netmap mode, all the work is done in the context
+	 * of the client thread. Interrupt handlers only wake up
+	 * clients, which may be sleeping on individual rings
+	 * or on a global resource for all rings.
+	 */
+	if (netmap_tx_irq(adapter->netdev, tx_ring->queue_index))
+		return 1; /* seems to be ignored */
+#endif /* DEV_NETMAP */
 	i = tx_ring->next_to_clean;
 	eop = tx_ring->tx_buffer_info[i].next_to_watch;
 	eop_desc = IXGBE_TX_DESC_ADV(tx_ring, eop);
@@ -1308,6 +1334,13 @@ static void ixgbe_clean_rx_irq(struct ixgbe_q_vector *q_vector,
 	u16 cleaned_count = 0;
 	bool pkt_is_rsc = false;
 
+#ifdef DEV_NETMAP
+	/*
+	 * Same as the txeof routine: only wakeup clients on intr.
+	 */
+	if (netmap_rx_irq(adapter->netdev, rx_ring->queue_index, work_done))
+		return;
+#endif /* DEV_NETMAP */
 	i = rx_ring->next_to_clean;
 	rx_desc = IXGBE_RX_DESC_ADV(rx_ring, i);
 	staterr = le32_to_cpu(rx_desc->wb.upper.status_error);
@@ -2730,6 +2763,9 @@ void ixgbe_configure_tx_ring(struct ixgbe_adapter *adapter,
 	} while (--wait_loop && !(txdctl & IXGBE_TXDCTL_ENABLE));
 	if (!wait_loop)
 		e_err(drv, "Could not enable Tx Queue %d\n", reg_idx);
+#ifdef DEV_NETMAP
+	ixgbe_netmap_configure_tx_ring(adapter, reg_idx);
+#endif /* DEV_NETMAP */
 }
 
 static void ixgbe_setup_mtqc(struct ixgbe_adapter *adapter)
@@ -3094,6 +3130,10 @@ void ixgbe_configure_rx_ring(struct ixgbe_adapter *adapter,
 	IXGBE_WRITE_REG(hw, IXGBE_RXDCTL(reg_idx), rxdctl);
 
 	ixgbe_rx_desc_queue_enable(adapter, ring);
+#ifdef DEV_NETMAP
+	if (ixgbe_netmap_configure_rx_ring(adapter, reg_idx))
+		return;
+#endif /* DEV_NETMAP */
 	ixgbe_alloc_rx_buffers(ring, IXGBE_DESC_UNUSED(ring));
 }
 
@@ -3882,6 +3922,10 @@ static int ixgbe_up_complete(struct ixgbe_adapter *adapter)
 	/* enable transmits */
 	netif_tx_start_all_queues(adapter->netdev);
 
+#ifdef DEV_NETMAP
+	netmap_enable_all_rings(adapter->netdev);
+#endif
+
 	/* bring the link up in the watchdog, this could race with our first
 	 * link up interrupt but shouldn't be a problem */
 	adapter->flags |= IXGBE_FLAG_NEED_LINK_UPDATE;
@@ -4121,6 +4165,10 @@ void ixgbe_down(struct ixgbe_adapter *adapter)
 
 	ixgbe_napi_disable_all(adapter);
 
+#ifdef DEV_NETMAP
+	netmap_disable_all_rings(netdev);
+#endif
+
 	/* Cleanup the affinity_hint CPU mask memory and callback */
 	for (i = 0; i < num_q_vectors; i++) {
 		struct ixgbe_q_vector *q_vector = adapter->q_vector[i];
@@ -7450,6 +7498,11 @@ static int __devinit ixgbe_probe(struct pci_dev *pdev,
 
 	e_dev_info("Intel(R) 10 Gigabit Network Connection\n");
 	cards_found++;
+
+#ifdef DEV_NETMAP
+	ixgbe_netmap_attach(adapter);
+#endif /* DEV_NETMAP */
+
 	return 0;
 
 err_register:
